Classes | Macros | Typedefs | Enumerations | Functions
ll_tim.h File Reference

Header file containing functions prototypes of TIMER LL library. More...

`#include "gr5x.h"`

Go to the source code of this file.

## Classes
struct | _ll_timer_capture_channel_init
| LL TIMER capture channel Structure definition. More...
struct | _ll_timer_init_t
| LL TIMER init Structure definition. More...

## Macros
#define | TIMER_DEFAULT_CONFIG
| LL TIMER InitStrcut default configuartion. More...
#define | LL_TIMER_INTSTAT_COUNTDONE TIMER_COUNTDONE_INT_STAT
| LL TIMER Interrupt source identify. More...
#define | LL_TIMER_INTSTAT_CH0 TIMER_CH0_INT_STAT
#define | LL_TIMER_INTSTAT_CH1 TIMER_CH1_INT_STAT
#define | LL_TIMER_INTSTAT_CH2 TIMER_CH2_INT_STAT
#define | LL_TIMER_INTSTAT_CH3 TIMER_CH3_INT_STAT
#define | LL_TIMER_INTSTAT_BLEPULSE1 TIMER_BLEPULSE1_INT_STAT
#define | LL_TIMER_INTSTAT_BLEPULSE2 TIMER_BLEPULSE2_INT_STAT
#define | LL_TIMER_WriteReg(__instance__, __REG__, __VALUE__) WRITE_REG(__instance__->__REG__, (__VALUE__))
| Write a value in TIMER register. More...
#define | LL_TIMER_ReadReg(__instance__, __REG__) READ_REG(__instance__->__REG__)
| Read a value in TIMER register. More...

## Typedefs
typedef struct _ll_timer_capture_channel_init | ll_timer_capture_channel_init_t
| LL TIMER capture channel Structure definition. More...
typedef struct _ll_timer_init_t | ll_timer_init_t
| LL TIMER init Structure definition. More...

## Enumerations
enum | ll_timer_capture_type_t { LL_TIMER_CAPTURE_NONE = 0x00, LL_TIMER_CAPTURE_FALLING = 0x01, LL_TIMER_CAPTURE_RISING = 0x02, LL_TIMER_CAPTURE_BOTH = 0x03 }
| LL TIMER capture type Enumerations definition. More...
enum | ll_timer_capture_pin_t { LL_TIMER_CAPTURE_IO0 = 0x00, LL_TIMER_CAPTURE_IO1 = 0x01, LL_TIMER_CAPTURE_IO2 = 0x02, LL_TIMER_CAPTURE_IO3 = 0x03, LL_TIMER_CAPTURE_IO4 = 0x04, LL_TIMER_CAPTURE_IO5 = 0x05, LL_TIMER_CAPTURE_IO6 = 0x06, LL_TIMER_CAPTURE_IO7 = 0x07, LL_TIMER_CAPTURE_IO8 = 0x08, LL_TIMER_CAPTURE_IO9 = 0x09, LL_TIMER_CAPTURE_IO10 = 0x0A, LL_TIMER_CAPTURE_IO11 = 0x0B, LL_TIMER_CAPTURE_IO12 = 0x0C, LL_TIMER_CAPTURE_IO13 = 0x0D, LL_TIMER_CAPTURE_IO14 = 0x0E, LL_TIMER_CAPTURE_IO15 = 0x0F, LL_TIMER_CAPTURE_IO16 = 0x10, LL_TIMER_CAPTURE_IO17 = 0x11, LL_TIMER_CAPTURE_IO18 = 0x12, LL_TIMER_CAPTURE_IO19 = 0x13, LL_TIMER_CAPTURE_IO20 = 0x14, LL_TIMER_CAPTURE_IO21 = 0x15, LL_TIMER_CAPTURE_IO22 = 0x16, LL_TIMER_CAPTURE_IO23 = 0x17, LL_TIMER_CAPTURE_IO24 = 0x18, LL_TIMER_CAPTURE_IO25 = 0x19, LL_TIMER_CAPTURE_IO26 = 0x1A, LL_TIMER_CAPTURE_IO27 = 0x1B, LL_TIMER_CAPTURE_IO28 = 0x1C, LL_TIMER_CAPTURE_IO29 = 0x1D, LL_TIMER_CAPTURE_IO30 = 0x1E, LL_TIMER_CAPTURE_IO31 = 0x1F }
| LL TIMER capture pin Enumerations definition. More...

## Functions
__STATIC_INLINE void | ll_timer_enable_counter (timer_regs_t *TIMERx)
| Enable timer counter. More...
__STATIC_INLINE void | ll_timer_disable_counter (timer_regs_t *TIMERx)
| Disable timer counter. More...
__STATIC_INLINE uint32_t | ll_timer_is_enabled_counter (timer_regs_t *TIMERx)
| Indicate whether the timer counter is enabled. More...
__STATIC_INLINE void | ll_timer_set_counter (timer_regs_t *TIMERx, uint32_t counter)
| Set the counter value. More...
__STATIC_INLINE uint32_t | ll_timer_get_counter (timer_regs_t *TIMERx)
| Get the counter value. More...
__STATIC_INLINE void | ll_timer_set_auto_reload (timer_regs_t *TIMERx, uint32_t auto_reload)
| Set the auto-reload value. More...
__STATIC_INLINE uint32_t | ll_timer_get_auto_reload (timer_regs_t *TIMERx)
| Get the auto-reload value. More...
__STATIC_INLINE void | ll_timer_enable_all_it (timer_regs_t *TIMERx)
| Enable timer all interrupt. More...
__STATIC_INLINE void | ll_timer_disable_all_it (timer_regs_t *TIMERx)
| Disable timer all interrput. More...
__STATIC_INLINE void | ll_timer_enable_countdone_it (timer_regs_t *TIMERx)
| Enable timer countdone interrupt. More...
__STATIC_INLINE void | ll_timer_disable_countdone_it (timer_regs_t *TIMERx)
| Disable timer countdone interrput. More...
__STATIC_INLINE void | ll_timer_enable_channel0_it (timer_regs_t *TIMERx)
| Enable timer channel0 interrupt. More...
__STATIC_INLINE void | ll_timer_disable_channel0_it (timer_regs_t *TIMERx)
| Disable timer channel0 interrput. More...
__STATIC_INLINE void | ll_timer_enable_channel1_it (timer_regs_t *TIMERx)
| Enable timer channel1 interrupt. More...
__STATIC_INLINE void | ll_timer_disable_channel1_it (timer_regs_t *TIMERx)
| Disable timer channel1 interrput. More...
__STATIC_INLINE void | ll_timer_enable_channel2_it (timer_regs_t *TIMERx)
| Enable timer channel2 interrupt. More...
__STATIC_INLINE void | ll_timer_disable_channel2_it (timer_regs_t *TIMERx)
| Disable timer channel2 interrput. More...
__STATIC_INLINE void | ll_timer_enable_channel3_it (timer_regs_t *TIMERx)
| Enable timer channel3 interrupt. More...
__STATIC_INLINE void | ll_timer_disable_channel3_it (timer_regs_t *TIMERx)
| Disable timer channel3 interrput. More...
__STATIC_INLINE void | ll_timer_enable_blepulse1_it (timer_regs_t *TIMERx)
| Enable timer ble pulse 1 interrupt. More...
__STATIC_INLINE void | ll_timer_disable_blepulse1_it (timer_regs_t *TIMERx)
| Disable timer ble pulse 1 interrput. More...
__STATIC_INLINE void | ll_timer_enable_blepulse2_it (timer_regs_t *TIMERx)
| Enable timer ble pulse 2 interrupt. More...
__STATIC_INLINE void | ll_timer_disable_blepulse2_it (timer_regs_t *TIMERx)
| Disable timer ble pulse 2 interrput. More...
__STATIC_INLINE uint32_t | ll_timer_is_enabled_it (timer_regs_t *TIMERx)
| Indicate whether the timer interrput is enabled. More...
__STATIC_INLINE void | ll_timer_clear_countdone_flag_it (timer_regs_t *TIMERx)
| Clear the COUNTDONE interrupt flag. More...
__STATIC_INLINE void | ll_timer_clear_channel0_flag_it (timer_regs_t *TIMERx)
| Clear the CHANNEL0 interrupt flag. More...
__STATIC_INLINE void | ll_timer_clear_channel1_flag_it (timer_regs_t *TIMERx)
| Clear the CHANNEL1 interrupt flag. More...
__STATIC_INLINE void | ll_timer_clear_channel2_flag_it (timer_regs_t *TIMERx)
| Clear the CHANNEL2 interrupt flag. More...
__STATIC_INLINE void | ll_timer_clear_channel3_flag_it (timer_regs_t *TIMERx)
| Clear the CHANNEL3 interrupt flag. More...
__STATIC_INLINE void | ll_timer_clear_blepulse1_flag_it (timer_regs_t *TIMERx)
| Clear the ble pulse 1 interrupt flag. More...
__STATIC_INLINE void | ll_timer_clear_blepulse2_flag_it (timer_regs_t *TIMERx)
| Clear the ble pulse 2 interrupt flag. More...
__STATIC_INLINE void | ll_timer_clear_all_flag_it (timer_regs_t *TIMERx)
| Clear the all interrupt flag. More...
__STATIC_INLINE uint32_t | ll_timer_is_active_flag_it (timer_regs_t *TIMERx)
| Indicate whether interrupt flag (INTSTAT) is set (interrupt is pending). More...
void | ll_timer_struct_init (ll_timer_init_t *p_timer_init)
| Set each field of a ll_timer_init_t type structure to default value. More...
__STATIC_INLINE void | ll_timer_set_channel0_capture_type (timer_regs_t *TIMERx, uint8_t ll_edge_capture)
| Set timer channel0 capture type. More...
__STATIC_INLINE ll_timer_capture_type_t | ll_timer_get_channel0_capture_type (timer_regs_t *TIMERx)
| Get timer channel0 capture type. More...
__STATIC_INLINE void | ll_timer_set_channel1_capture_type (timer_regs_t *TIMERx, uint8_t ll_edge_capture)
| Set timer channel1 capture type. More...
__STATIC_INLINE ll_timer_capture_type_t | ll_timer_get_channel1_capture_type (timer_regs_t *TIMERx)
| Get timer channel1 capture type. More...
__STATIC_INLINE void | ll_timer_set_channel2_capture_type (timer_regs_t *TIMERx, uint8_t ll_edge_capture)
| Set timer channel2 capture type. More...
__STATIC_INLINE ll_timer_capture_type_t | ll_timer_get_channel2_capture_type (timer_regs_t *TIMERx)
| Get timer channel2 capture type. More...
__STATIC_INLINE void | ll_timer_set_channel3_capture_type (timer_regs_t *TIMERx, uint8_t ll_edge_capture)
| Set timer channel3 capture type. More...
__STATIC_INLINE ll_timer_capture_type_t | ll_timer_get_channel3_capture_type (timer_regs_t *TIMERx)
| Get timer channel3 capture type. More...
__STATIC_INLINE void | ll_timer_set_channel0_capture_pin (timer_regs_t *TIMERx, uint8_t ll_capture_pin)
| Set timer channel0 capture pin. More...
__STATIC_INLINE ll_timer_capture_pin_t | ll_timer_get_channel0_capture_pin (timer_regs_t *TIMERx)
| Get timer channel0 capture pin. More...
__STATIC_INLINE void | ll_timer_set_channel1_capture_pin (timer_regs_t *TIMERx, uint8_t ll_capture_pin)
| Set timer channel1 capture pin. More...
__STATIC_INLINE ll_timer_capture_pin_t | ll_timer_get_channel1_capture_pin (timer_regs_t *TIMERx)
| Get timer channel1 capture pin. More...
__STATIC_INLINE void | ll_timer_set_channel2_capture_pin (timer_regs_t *TIMERx, uint8_t ll_capture_pin)
| Set timer channel2 capture pin. More...
__STATIC_INLINE ll_timer_capture_pin_t | ll_timer_get_channel2_capture_pin (timer_regs_t *TIMERx)
| Get timer channel2 capture pin. More...
__STATIC_INLINE void | ll_timer_set_channel3_capture_pin (timer_regs_t *TIMERx, uint8_t ll_capture_pin)
| Set timer channel3 capture pin. More...
__STATIC_INLINE ll_timer_capture_pin_t | ll_timer_get_channel3_capture_pin (timer_regs_t *TIMERx)
| Get timer channel3 capture pin. More...
__STATIC_INLINE uint32_t | ll_timer_get_it_flag (timer_regs_t *TIMERx)
| Get timer interrupt flag. More...
__STATIC_INLINE uint32_t | ll_timer_get_channel0_val (timer_regs_t *TIMERx)
| Get current value of channel0. More...
__STATIC_INLINE uint32_t | ll_timer_get_channel1_val (timer_regs_t *TIMERx)
| Get current value of channel1. More...
__STATIC_INLINE uint32_t | ll_timer_get_channel2_val (timer_regs_t *TIMERx)
| Get current value of channel2. More...
__STATIC_INLINE uint32_t | ll_timer_get_channel3_val (timer_regs_t *TIMERx)
| Get current value of channel3. More...
__STATIC_INLINE void | ll_timer_enable_ble_pulse (timer_regs_t *TIMERx)
| Enable timer BLE pulse. More...
__STATIC_INLINE void | ll_timer_disable_ble_pulse (timer_regs_t *TIMERx)
| Disable timer BLE pulse. More...
__STATIC_INLINE uint32_t | ll_timer_is_enabled_ble_pulse (timer_regs_t *TIMERx)
| Indicate whether the timer BLE pulse is enabled. More...
__STATIC_INLINE void | ll_timer_set_BLE_val1 (timer_regs_t *TIMERx, uint32_t value)
| Set the BLE count value1. More...
__STATIC_INLINE uint32_t | ll_timer_get_BLE_val1 (timer_regs_t *TIMERx)
| Get the BLE count value1. More...
__STATIC_INLINE void | ll_timer_set_BLE_val2 (timer_regs_t *TIMERx, uint32_t value)
| Set the BLE count value2. More...
__STATIC_INLINE uint32_t | ll_timer_get_BLE_val2 (timer_regs_t *TIMERx)
| Get the BLE count value2. More...
__STATIC_INLINE void | ll_timer_set_BLE_pulse_width (timer_regs_t *TIMERx, uint32_t width)
| Set the BLE pulse width. More...
__STATIC_INLINE uint32_t | ll_timer_get_pulse_width (timer_regs_t *TIMERx)
| Get the BLE pulse width. More...

## Detailed Description

Header file containing functions prototypes of TIMER LL library.

Author
  BLE Driver Team

Attention
  #####Copyright (c) 2019 GOODIX All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file ll_tim.h.