Classes | Typedefs | Enumerations
TIMER Exported init structures
Peripheral Driver » LL Driver » TIMER » Structures

## Classes
struct | _ll_timer_capture_channel_init
| LL TIMER capture channel Structure definition. More...
struct | _ll_timer_init_t
| LL TIMER init Structure definition. More...

## Typedefs
typedef struct _ll_timer_capture_channel_init | ll_timer_capture_channel_init_t
| LL TIMER capture channel Structure definition. More...
typedef struct _ll_timer_init_t | ll_timer_init_t
| LL TIMER init Structure definition. More...

## Enumerations
enum | ll_timer_capture_type_t { LL_TIMER_CAPTURE_NONE = 0x00, LL_TIMER_CAPTURE_FALLING = 0x01, LL_TIMER_CAPTURE_RISING = 0x02, LL_TIMER_CAPTURE_BOTH = 0x03 }
| LL TIMER capture type Enumerations definition. More...
enum | ll_timer_capture_pin_t { LL_TIMER_CAPTURE_IO0 = 0x00, LL_TIMER_CAPTURE_IO1 = 0x01, LL_TIMER_CAPTURE_IO2 = 0x02, LL_TIMER_CAPTURE_IO3 = 0x03, LL_TIMER_CAPTURE_IO4 = 0x04, LL_TIMER_CAPTURE_IO5 = 0x05, LL_TIMER_CAPTURE_IO6 = 0x06, LL_TIMER_CAPTURE_IO7 = 0x07, LL_TIMER_CAPTURE_IO8 = 0x08, LL_TIMER_CAPTURE_IO9 = 0x09, LL_TIMER_CAPTURE_IO10 = 0x0A, LL_TIMER_CAPTURE_IO11 = 0x0B, LL_TIMER_CAPTURE_IO12 = 0x0C, LL_TIMER_CAPTURE_IO13 = 0x0D, LL_TIMER_CAPTURE_IO14 = 0x0E, LL_TIMER_CAPTURE_IO15 = 0x0F, LL_TIMER_CAPTURE_IO16 = 0x10, LL_TIMER_CAPTURE_IO17 = 0x11, LL_TIMER_CAPTURE_IO18 = 0x12, LL_TIMER_CAPTURE_IO19 = 0x13, LL_TIMER_CAPTURE_IO20 = 0x14, LL_TIMER_CAPTURE_IO21 = 0x15, LL_TIMER_CAPTURE_IO22 = 0x16, LL_TIMER_CAPTURE_IO23 = 0x17, LL_TIMER_CAPTURE_IO24 = 0x18, LL_TIMER_CAPTURE_IO25 = 0x19, LL_TIMER_CAPTURE_IO26 = 0x1A, LL_TIMER_CAPTURE_IO27 = 0x1B, LL_TIMER_CAPTURE_IO28 = 0x1C, LL_TIMER_CAPTURE_IO29 = 0x1D, LL_TIMER_CAPTURE_IO30 = 0x1E, LL_TIMER_CAPTURE_IO31 = 0x1F }
| LL TIMER capture pin Enumerations definition. More...

## Detailed Description

## Typedef Documentation

## ◆ ll_timer_capture_channel_init_t

typedef struct _ll_timer_capture_channel_init ll_timer_capture_channel_init_t

LL TIMER capture channel Structure definition.

## ◆ ll_timer_init_t

typedef struct _ll_timer_init_t ll_timer_init_t

LL TIMER init Structure definition.

## Enumeration Type Documentation

## ◆ ll_timer_capture_pin_t

enum ll_timer_capture_pin_t

LL TIMER capture pin Enumerations definition.

Enumerator
LL_TIMER_CAPTURE_IO0 | capture IO0
LL_TIMER_CAPTURE_IO1 | capture IO1
LL_TIMER_CAPTURE_IO2 | capture IO2
LL_TIMER_CAPTURE_IO3 | capture IO3
LL_TIMER_CAPTURE_IO4 | capture IO4
LL_TIMER_CAPTURE_IO5 | capture IO5
LL_TIMER_CAPTURE_IO6 | capture IO6
LL_TIMER_CAPTURE_IO7 | capture IO7
LL_TIMER_CAPTURE_IO8 | capture IO8
LL_TIMER_CAPTURE_IO9 | capture IO9
LL_TIMER_CAPTURE_IO10 | capture IO10
LL_TIMER_CAPTURE_IO11 | capture IO11
LL_TIMER_CAPTURE_IO12 | capture IO12
LL_TIMER_CAPTURE_IO13 | capture IO13
LL_TIMER_CAPTURE_IO14 | capture IO14
LL_TIMER_CAPTURE_IO15 | capture IO15
LL_TIMER_CAPTURE_IO16 | capture IO16
LL_TIMER_CAPTURE_IO17 | capture IO17
LL_TIMER_CAPTURE_IO18 | capture IO18
LL_TIMER_CAPTURE_IO19 | capture IO19
LL_TIMER_CAPTURE_IO20 | capture IO20
LL_TIMER_CAPTURE_IO21 | capture IO21
LL_TIMER_CAPTURE_IO22 | capture IO22
LL_TIMER_CAPTURE_IO23 | capture IO23
LL_TIMER_CAPTURE_IO24 | capture IO24
LL_TIMER_CAPTURE_IO25 | capture IO25
LL_TIMER_CAPTURE_IO26 | capture IO26
LL_TIMER_CAPTURE_IO27 | capture IO27
LL_TIMER_CAPTURE_IO28 | capture IO28
LL_TIMER_CAPTURE_IO29 | capture IO29
LL_TIMER_CAPTURE_IO30 | capture IO30
LL_TIMER_CAPTURE_IO31 | capture IO31

Definition at line 87 of file ll_tim.h.

## ◆ ll_timer_capture_type_t

enum ll_timer_capture_type_t

LL TIMER capture type Enumerations definition.

Enumerator
LL_TIMER_CAPTURE_NONE | Set timer capture NONE
LL_TIMER_CAPTURE_FALLING | Set timer capture io falling edge
LL_TIMER_CAPTURE_RISING | Set timer capture io rising edge
LL_TIMER_CAPTURE_BOTH | Set timer capture io both edge

Definition at line 76 of file ll_tim.h.