Macros
Individual block's clock control inside security system
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

## Macros
#define | LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_FORCE_OFF
#define | LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_SLP_OFF
#define | LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_FORCE_OFF
#define | LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_SLP_OFF
#define | LL_CGC_MCU_SECU_FRC_OFF_HCLK ((uint32_t)0x00001400U)
#define | LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK ((uint32_t)0x00002800U)
#define | LL_CGC_MCU_SECU_FRC_OFF_ALL

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN

#define LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_FORCE_OFF

Force individual efuse's clock control

Definition at line 174 of file ll_cgc.h.

## ◆ LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN

#define LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_FORCE_OFF

Force individual rng's clock control

Definition at line 172 of file ll_cgc.h.

## ◆ LL_CGC_MCU_SECU_FRC_OFF_ALL

#define LL_CGC_MCU_SECU_FRC_OFF_ALL

Value:
(LL_CGC_MCU_SECU_FRC_OFF_HCLK |\
LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK)

Hclk for security clock

Definition at line 181 of file ll_cgc.h.

## ◆ LL_CGC_MCU_SECU_FRC_OFF_HCLK

#define LL_CGC_MCU_SECU_FRC_OFF_HCLK ((uint32_t)0x00001400U)

Hclk for security clock

Definition at line 177 of file ll_cgc.h.

## ◆ LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK

#define LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK ((uint32_t)0x00002800U)

Hclk for security clock WFI/WFE

Definition at line 178 of file ll_cgc.h.

## ◆ LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN

#define LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_SLP_OFF

Individual efuse's clock control

Definition at line 175 of file ll_cgc.h.

## ◆ LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN

#define LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_SLP_OFF

Individual rng's clock control

Definition at line 173 of file ll_cgc.h.

LL_CGC_MCU_SECU_FRC_OFF_HCLK
#define LL_CGC_MCU_SECU_FRC_OFF_HCLK
Definition: ll_cgc.h:177