Public Attributes | List of all members
_pkc_montgomery_multi Struct Reference
Peripheral Driver » HAL Driver » PKC » Structures » PKC expression input

PKC Montgomery Modular Multiplication expression input. More...

`#include <hal_pkc.h>`

## Public Attributes
uint32_t * | p_A
uint32_t * | p_B
uint32_t * | p_P
uint32_t | ConstP

## Detailed Description

PKC Montgomery Modular Multiplication expression input.

Note
  Result = A * B * R^(-1) mod P, where R = 2^DataBits

Definition at line 212 of file hal_pkc.h.

## Member Data Documentation

## ◆ ConstP

uint32_t _pkc_montgomery_multi::ConstP

Montgomery multiplication constant for P, where constp = (-P[0])^(-1) mod 2^32

Definition at line 217 of file hal_pkc.h.

## ◆ p_A

uint32_t* _pkc_montgomery_multi::p_A

Pointer to operand A

Definition at line 214 of file hal_pkc.h.

## ◆ p_B

uint32_t* _pkc_montgomery_multi::p_B

Pointer to operand B

Definition at line 215 of file hal_pkc.h.

## ◆ p_P

uint32_t* _pkc_montgomery_multi::p_P

Pointer to prime number P

Definition at line 216 of file hal_pkc.h.

The documentation for this struct was generated from the following file:

- hal_pkc.h