Public Attributes | List of all members
gatts_write_req_cb_t Struct Reference
BLE » Profile » Profile Server » Structures

GATT write request struct. More...

`#include <ble_prf.h>`

## Public Attributes
uint16_t | handle
uint16_t | offset
uint16_t | length
uint8_t | value [__ARRAY_EMPTY]

## Detailed Description

GATT write request struct.

Definition at line 136 of file ble_prf.h.

## Member Data Documentation

## ◆ handle

uint16_t gatts_write_req_cb_t::handle

Handle of the attribute to be written.

Definition at line 138 of file ble_prf.h.

## ◆ length

uint16_t gatts_write_req_cb_t::length

Data length to be written.

Definition at line 140 of file ble_prf.h.

## ◆ offset

uint16_t gatts_write_req_cb_t::offset

Offset at which the data has to be written.

Definition at line 139 of file ble_prf.h.

## ◆ value

uint8_t gatts_write_req_cb_t::value[__ARRAY_EMPTY]

Data to be written to characteristic value.

Definition at line 141 of file ble_prf.h.

The documentation for this struct was generated from the following file:

- ble_prf.h