Macros
SPI Data Size
Peripheral Driver » HAL Driver » SPI » CS Signal Description » Defines » SPI Exported Constants

## Macros
#define | SPI_DATASIZE_4BIT LL_SPI_DATASIZE_4BIT
#define | SPI_DATASIZE_5BIT LL_SPI_DATASIZE_5BIT
#define | SPI_DATASIZE_6BIT LL_SPI_DATASIZE_6BIT
#define | SPI_DATASIZE_7BIT LL_SPI_DATASIZE_7BIT
#define | SPI_DATASIZE_8BIT LL_SPI_DATASIZE_8BIT
#define | SPI_DATASIZE_9BIT LL_SPI_DATASIZE_9BIT
#define | SPI_DATASIZE_10BIT LL_SPI_DATASIZE_10BIT
#define | SPI_DATASIZE_11BIT LL_SPI_DATASIZE_11BIT
#define | SPI_DATASIZE_12BIT LL_SPI_DATASIZE_12BIT
#define | SPI_DATASIZE_13BIT LL_SPI_DATASIZE_13BIT
#define | SPI_DATASIZE_14BIT LL_SPI_DATASIZE_14BIT
#define | SPI_DATASIZE_15BIT LL_SPI_DATASIZE_15BIT
#define | SPI_DATASIZE_16BIT LL_SPI_DATASIZE_16BIT
#define | SPI_DATASIZE_17BIT LL_SPI_DATASIZE_17BIT
#define | SPI_DATASIZE_18BIT LL_SPI_DATASIZE_18BIT
#define | SPI_DATASIZE_19BIT LL_SPI_DATASIZE_19BIT
#define | SPI_DATASIZE_20BIT LL_SPI_DATASIZE_20BIT
#define | SPI_DATASIZE_21BIT LL_SPI_DATASIZE_21BIT
#define | SPI_DATASIZE_22BIT LL_SPI_DATASIZE_22BIT
#define | SPI_DATASIZE_23BIT LL_SPI_DATASIZE_23BIT
#define | SPI_DATASIZE_24BIT LL_SPI_DATASIZE_24BIT
#define | SPI_DATASIZE_25BIT LL_SPI_DATASIZE_25BIT
#define | SPI_DATASIZE_26BIT LL_SPI_DATASIZE_26BIT
#define | SPI_DATASIZE_27BIT LL_SPI_DATASIZE_27BIT
#define | SPI_DATASIZE_28BIT LL_SPI_DATASIZE_28BIT
#define | SPI_DATASIZE_29BIT LL_SPI_DATASIZE_29BIT
#define | SPI_DATASIZE_30BIT LL_SPI_DATASIZE_30BIT
#define | SPI_DATASIZE_31BIT LL_SPI_DATASIZE_31BIT
#define | SPI_DATASIZE_32BIT LL_SPI_DATASIZE_32BIT

## Detailed Description

## Macro Definition Documentation

## ◆ SPI_DATASIZE_10BIT

#define SPI_DATASIZE_10BIT LL_SPI_DATASIZE_10BIT

10-bit serial data transfer

Definition at line 303 of file hal_spi.h.

## ◆ SPI_DATASIZE_11BIT

#define SPI_DATASIZE_11BIT LL_SPI_DATASIZE_11BIT

11-bit serial data transfer

Definition at line 304 of file hal_spi.h.

## ◆ SPI_DATASIZE_12BIT

#define SPI_DATASIZE_12BIT LL_SPI_DATASIZE_12BIT

12-bit serial data transfer

Definition at line 305 of file hal_spi.h.

## ◆ SPI_DATASIZE_13BIT

#define SPI_DATASIZE_13BIT LL_SPI_DATASIZE_13BIT

13-bit serial data transfer

Definition at line 306 of file hal_spi.h.

## ◆ SPI_DATASIZE_14BIT

#define SPI_DATASIZE_14BIT LL_SPI_DATASIZE_14BIT

14-bit serial data transfer

Definition at line 307 of file hal_spi.h.

## ◆ SPI_DATASIZE_15BIT

#define SPI_DATASIZE_15BIT LL_SPI_DATASIZE_15BIT

15-bit serial data transfer

Definition at line 308 of file hal_spi.h.

## ◆ SPI_DATASIZE_16BIT

#define SPI_DATASIZE_16BIT LL_SPI_DATASIZE_16BIT

16-bit serial data transfer

Definition at line 309 of file hal_spi.h.

## ◆ SPI_DATASIZE_17BIT

#define SPI_DATASIZE_17BIT LL_SPI_DATASIZE_17BIT

17-bit serial data transfer

Definition at line 310 of file hal_spi.h.

## ◆ SPI_DATASIZE_18BIT

#define SPI_DATASIZE_18BIT LL_SPI_DATASIZE_18BIT

18-bit serial data transfer

Definition at line 311 of file hal_spi.h.

## ◆ SPI_DATASIZE_19BIT

#define SPI_DATASIZE_19BIT LL_SPI_DATASIZE_19BIT

19-bit serial data transfer

Definition at line 312 of file hal_spi.h.

## ◆ SPI_DATASIZE_20BIT

#define SPI_DATASIZE_20BIT LL_SPI_DATASIZE_20BIT

20-bit serial data transfer

Definition at line 313 of file hal_spi.h.

## ◆ SPI_DATASIZE_21BIT

#define SPI_DATASIZE_21BIT LL_SPI_DATASIZE_21BIT

21-bit serial data transfer

Definition at line 314 of file hal_spi.h.

## ◆ SPI_DATASIZE_22BIT

#define SPI_DATASIZE_22BIT LL_SPI_DATASIZE_22BIT

22-bit serial data transfer

Definition at line 315 of file hal_spi.h.

## ◆ SPI_DATASIZE_23BIT

#define SPI_DATASIZE_23BIT LL_SPI_DATASIZE_23BIT

23-bit serial data transfer

Definition at line 316 of file hal_spi.h.

## ◆ SPI_DATASIZE_24BIT

#define SPI_DATASIZE_24BIT LL_SPI_DATASIZE_24BIT

24-bit serial data transfer

Definition at line 317 of file hal_spi.h.

## ◆ SPI_DATASIZE_25BIT

#define SPI_DATASIZE_25BIT LL_SPI_DATASIZE_25BIT

25-bit serial data transfer

Definition at line 318 of file hal_spi.h.

## ◆ SPI_DATASIZE_26BIT

#define SPI_DATASIZE_26BIT LL_SPI_DATASIZE_26BIT

26-bit serial data transfer

Definition at line 319 of file hal_spi.h.

## ◆ SPI_DATASIZE_27BIT

#define SPI_DATASIZE_27BIT LL_SPI_DATASIZE_27BIT

27-bit serial data transfer

Definition at line 320 of file hal_spi.h.

## ◆ SPI_DATASIZE_28BIT

#define SPI_DATASIZE_28BIT LL_SPI_DATASIZE_28BIT

28-bit serial data transfer

Definition at line 321 of file hal_spi.h.

## ◆ SPI_DATASIZE_29BIT

#define SPI_DATASIZE_29BIT LL_SPI_DATASIZE_29BIT

29-bit serial data transfer

Definition at line 322 of file hal_spi.h.

## ◆ SPI_DATASIZE_30BIT

#define SPI_DATASIZE_30BIT LL_SPI_DATASIZE_30BIT

30-bit serial data transfer

Definition at line 323 of file hal_spi.h.

## ◆ SPI_DATASIZE_31BIT

#define SPI_DATASIZE_31BIT LL_SPI_DATASIZE_31BIT

31-bit serial data transfer

Definition at line 324 of file hal_spi.h.

## ◆ SPI_DATASIZE_32BIT

#define SPI_DATASIZE_32BIT LL_SPI_DATASIZE_32BIT

32-bit serial data transfer

Definition at line 325 of file hal_spi.h.

## ◆ SPI_DATASIZE_4BIT

#define SPI_DATASIZE_4BIT LL_SPI_DATASIZE_4BIT

4-bit serial data transfer

Definition at line 297 of file hal_spi.h.

## ◆ SPI_DATASIZE_5BIT

#define SPI_DATASIZE_5BIT LL_SPI_DATASIZE_5BIT

5-bit serial data transfer

Definition at line 298 of file hal_spi.h.

## ◆ SPI_DATASIZE_6BIT

#define SPI_DATASIZE_6BIT LL_SPI_DATASIZE_6BIT

6-bit serial data transfer

Definition at line 299 of file hal_spi.h.

## ◆ SPI_DATASIZE_7BIT

#define SPI_DATASIZE_7BIT LL_SPI_DATASIZE_7BIT

7-bit serial data transfer

Definition at line 300 of file hal_spi.h.

## ◆ SPI_DATASIZE_8BIT

#define SPI_DATASIZE_8BIT LL_SPI_DATASIZE_8BIT

8-bit serial data transfer

Definition at line 301 of file hal_spi.h.

## ◆ SPI_DATASIZE_9BIT

#define SPI_DATASIZE_9BIT LL_SPI_DATASIZE_9BIT

9-bit serial data transfer

Definition at line 302 of file hal_spi.h.