Macros
DMA request definitions
Peripheral Driver » HAL Driver » DMA » Defines » DMA Exported Constants

## Macros
#define | DMA0_REQUEST_CTE LL_DMA0_PERIPH_CTE
#define | DMA0_REQUEST_PWM0 LL_DMA0_PERIPH_PWM0
#define | DMA0_REQUEST_SPIM_TX LL_DMA0_PERIPH_SPIM_TX
#define | DMA0_REQUEST_SPIM_RX LL_DMA0_PERIPH_SPIM_RX
#define | DMA0_REQUEST_SPIS_TX LL_DMA0_PERIPH_SPIS_TX
#define | DMA0_REQUEST_SPIS_RX LL_DMA0_PERIPH_SPIS_RX
#define | DMA0_REQUEST_UART0_TX LL_DMA0_PERIPH_UART0_TX
#define | DMA0_REQUEST_UART0_RX LL_DMA0_PERIPH_UART0_RX
#define | DMA0_REQUEST_UART1_TX LL_DMA0_PERIPH_UART1_TX
#define | DMA0_REQUEST_UART1_RX LL_DMA0_PERIPH_UART1_RX
#define | DMA0_REQUEST_SNSADC LL_DMA0_PERIPH_SNSADC
#define | DMA0_REQUEST_I2C0_TX LL_DMA0_PERIPH_I2C0_TX
#define | DMA0_REQUEST_I2C0_RX LL_DMA0_PERIPH_I2C0_RX
#define | DMA0_REQUEST_I2C1_TX LL_DMA0_PERIPH_I2C1_TX
#define | DMA0_REQUEST_I2C1_RX LL_DMA0_PERIPH_I2C1_RX
#define | DMA0_REQUEST_MEM LL_DMA0_PERIPH_MEM

## Detailed Description

## Macro Definition Documentation

## ◆ DMA0_REQUEST_CTE

#define DMA0_REQUEST_CTE LL_DMA0_PERIPH_CTE

DMA CTE transmit request

Definition at line 245 of file hal_dma.h.

## ◆ DMA0_REQUEST_I2C0_RX

#define DMA0_REQUEST_I2C0_RX LL_DMA0_PERIPH_I2C0_RX

DMA peripheral type is I2C0 RX

Definition at line 257 of file hal_dma.h.

## ◆ DMA0_REQUEST_I2C0_TX

#define DMA0_REQUEST_I2C0_TX LL_DMA0_PERIPH_I2C0_TX

DMA peripheral type is I2C0 TX

Definition at line 256 of file hal_dma.h.

## ◆ DMA0_REQUEST_I2C1_RX

#define DMA0_REQUEST_I2C1_RX LL_DMA0_PERIPH_I2C1_RX

DMA peripheral type is I2C1 RX

Definition at line 259 of file hal_dma.h.

## ◆ DMA0_REQUEST_I2C1_TX

#define DMA0_REQUEST_I2C1_TX LL_DMA0_PERIPH_I2C1_TX

DMA peripheral type is I2C1 TX

Definition at line 258 of file hal_dma.h.

## ◆ DMA0_REQUEST_MEM

#define DMA0_REQUEST_MEM LL_DMA0_PERIPH_MEM

DMA is Memory transmit request

Definition at line 260 of file hal_dma.h.

## ◆ DMA0_REQUEST_PWM0

#define DMA0_REQUEST_PWM0 LL_DMA0_PERIPH_PWM0

DMA PWM0 transmit request

Definition at line 246 of file hal_dma.h.

## ◆ DMA0_REQUEST_SNSADC

#define DMA0_REQUEST_SNSADC LL_DMA0_PERIPH_SNSADC

DMA SNSADC transmit request

Definition at line 255 of file hal_dma.h.

## ◆ DMA0_REQUEST_SPIM_RX

#define DMA0_REQUEST_SPIM_RX LL_DMA0_PERIPH_SPIM_RX

DMA SPIM RX transmit request

Definition at line 248 of file hal_dma.h.

## ◆ DMA0_REQUEST_SPIM_TX

#define DMA0_REQUEST_SPIM_TX LL_DMA0_PERIPH_SPIM_TX

DMA SPIM transmit request

Definition at line 247 of file hal_dma.h.

## ◆ DMA0_REQUEST_SPIS_RX

#define DMA0_REQUEST_SPIS_RX LL_DMA0_PERIPH_SPIS_RX

DMA SPIS RX transmit request

Definition at line 250 of file hal_dma.h.

## ◆ DMA0_REQUEST_SPIS_TX

#define DMA0_REQUEST_SPIS_TX LL_DMA0_PERIPH_SPIS_TX

DMA SPIS TX transmit request

Definition at line 249 of file hal_dma.h.

## ◆ DMA0_REQUEST_UART0_RX

#define DMA0_REQUEST_UART0_RX LL_DMA0_PERIPH_UART0_RX

DMA UART0 RX transmit request

Definition at line 252 of file hal_dma.h.

## ◆ DMA0_REQUEST_UART0_TX

#define DMA0_REQUEST_UART0_TX LL_DMA0_PERIPH_UART0_TX

DMA UART0 TX transmit request

Definition at line 251 of file hal_dma.h.

## ◆ DMA0_REQUEST_UART1_RX

#define DMA0_REQUEST_UART1_RX LL_DMA0_PERIPH_UART1_RX

DMA UART1 RX transmit request

Definition at line 254 of file hal_dma.h.

## ◆ DMA0_REQUEST_UART1_TX

#define DMA0_REQUEST_UART1_TX LL_DMA0_PERIPH_UART1_TX

DMA UART1 TX transmit request

Definition at line 253 of file hal_dma.h.