Macros
Clock divider
Peripheral Driver » LL Driver » RTC » Defines » RTC Exported Constants

## Macros
#define | LL_RTC_DIV_NONE ((uint32_t)0x00U)
#define | LL_RTC_DIV_2 ((uint32_t)0x01UL << RTC_CFG1_DIV_Pos)
#define | LL_RTC_DIV_4 ((uint32_t)0x02UL << RTC_CFG1_DIV_Pos)
#define | LL_RTC_DIV_8 ((uint32_t)0x03UL << RTC_CFG1_DIV_Pos)
#define | LL_RTC_DIV_16 ((uint32_t)0x04UL << RTC_CFG1_DIV_Pos)
#define | LL_RTC_DIV_32 ((uint32_t)0x05UL << RTC_CFG1_DIV_Pos)
#define | LL_RTC_DIV_64 ((uint32_t)0x06UL << RTC_CFG1_DIV_Pos)
#define | LL_RTC_DIV_128 ((uint32_t)0x07UL << RTC_CFG1_DIV_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_RTC_DIV_128

#define LL_RTC_DIV_128 ((uint32_t)0x07UL << RTC_CFG1_DIV_Pos)

Select 1/256 divider

Definition at line 80 of file ll_rtc.h.

## ◆ LL_RTC_DIV_16

#define LL_RTC_DIV_16 ((uint32_t)0x04UL << RTC_CFG1_DIV_Pos)

Select 1/32 divider

Definition at line 77 of file ll_rtc.h.

## ◆ LL_RTC_DIV_2

#define LL_RTC_DIV_2 ((uint32_t)0x01UL << RTC_CFG1_DIV_Pos)

Select 1/32 divider

Definition at line 74 of file ll_rtc.h.

## ◆ LL_RTC_DIV_32

#define LL_RTC_DIV_32 ((uint32_t)0x05UL << RTC_CFG1_DIV_Pos)

Select 1/64 divider

Definition at line 78 of file ll_rtc.h.

## ◆ LL_RTC_DIV_4

#define LL_RTC_DIV_4 ((uint32_t)0x02UL << RTC_CFG1_DIV_Pos)

Select 1/32 divider

Definition at line 75 of file ll_rtc.h.

## ◆ LL_RTC_DIV_64

#define LL_RTC_DIV_64 ((uint32_t)0x06UL << RTC_CFG1_DIV_Pos)

Select 1/128 divider

Definition at line 79 of file ll_rtc.h.

## ◆ LL_RTC_DIV_8

#define LL_RTC_DIV_8 ((uint32_t)0x03UL << RTC_CFG1_DIV_Pos)

Select 1/32 divider

Definition at line 76 of file ll_rtc.h.

## ◆ LL_RTC_DIV_NONE

#define LL_RTC_DIV_NONE ((uint32_t)0x00U)

Select SLP_CLK

Definition at line 73 of file ll_rtc.h.