Macros
Own Address Length
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants

## Macros
#define | LL_I2C_OWNADDRESS_7BIT 0x00000000U
#define | LL_I2C_OWNADDRESS_10BIT I2C_CTRL_ADDR_BIT_S

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_OWNADDRESS_10BIT

#define LL_I2C_OWNADDRESS_10BIT I2C_CTRL_ADDR_BIT_S

Own address 1 is a 10-bit address.

Definition at line 180 of file ll_i2c.h.

## ◆ LL_I2C_OWNADDRESS_7BIT

#define LL_I2C_OWNADDRESS_7BIT 0x00000000U

Own address 1 is a 7-bit address.

Definition at line 179 of file ll_i2c.h.